Woven railroad directions   Quilt show challenge for 2027
Diane Mitchell /509-679-8071
*Choose any railroad car of your preference; box car, tanker, coal carrier, auto carrier, passenger, engine, container carrier, etc.  Graffiti optional.  Make the railcar 16 -17” long
*Show the side and a suggestion of the end of the car ie. 2 sides of the railcar. The second side should be on the righthand side of the piece as if the train is moving away from your view. 
*Finished size 12”x 18” with a facing finish preferred to a binding finish
*Use a recognizable piece of provided fabric on the front of the piece. You may dye, embellish, paint or otherwise change fabric color. Its beet season; beet juice makes a great dye.
*Railroad track material used needs to lay 2” from the bottom of the piece. I found grey seam tape topped by ¼” bias binding looked pretty realistic.
Construction suggestions:
 Cut a 14x 20” piece of fusible batting and iron it to your backing fabric.  This will let you trim it to size once the pieces have been added. Size shrinks with fabric manipulation. Build sky and foreground before applying the body of the railcar.  Consider a second layer of batting beneath the railcar body for depth.  When you have your assembly finished and everything pressed flat then trim to a 12 ½”x18 ½” size. Apply facing material and turn under the ¼” seam allowances to finish.

If you think we need a class on it let the workshops person know or ask Diane for help.
